# **A confocal micro-Raman spectroscopy system for microplastics detection, combined with IoT.**

**Introduction**

[Micro-Raman spectroscopy is a technique that combines Raman spectroscopy with a traditional light microscope1](https://www.bruker.com/en/products-and-solutions/infrared-and-raman/raman-microscopes/what-is-raman-microscopy.html). [This allows for the chemical analysis of very tiny objects](https://www.bruker.com/en/products-and-solutions/infrared-and-raman/raman-microscopes/what-is-raman-microscopy.html). [The system works by illuminating the sample with a laser, which interacts with the sample and scatters off its surface](https://www.bruker.com/en/products-and-solutions/infrared-and-raman/raman-microscopes/what-is-raman-microscopy.html). [The scattered light is then detected to create a Raman spectrum, which acts as a unique “chemical fingerprint” for the compounds present in the sample](https://www.bruker.com/en/products-and-solutions/infrared-and-raman/raman-microscopes/what-is-raman-microscopy.html).

[In confocal micro-Raman spectroscopy, a spatial filter is used to control the analysis volume of the sample in the XY (lateral) and Z (depth) axes](https://www.horiba.com/int/scientific/technologies/raman-imaging-and-spectroscopy/confocal-raman-microscopy/). [This allows for high-resolution analysis of individual particles or layers with dimensions as low as 1 µm](https://www.horiba.com/int/scientific/technologies/raman-imaging-and-spectroscopy/confocal-raman-microscopy/).

* **Sensors and Devices**: These are attached to the confocal micro-Raman spectroscopy system to collect data. [They can vary widely, from simple temperature sensors to sophisticated multi-functional devices that measure a range of variables](https://telnyx.com/resources/iot-remote-monitoring).
* **Connectivity:** This involves various communication protocols like Wi-Fi, Bluetooth, and cellular networks. [The IoT device communicates with the cloud server via Wi-Fi, allowing for remote monitoring and control of the system](https://telnyx.com/resources/iot-remote-monitoring).
* **Data Processing and Analysis:** Advanced algorithms, like machine learning models, process and analyze the collected data. [This step turns raw data into actionable insights](https://telnyx.com/resources/iot-remote-monitoring).
* [**Cloud Server:** The data collected by the confocal micro-Raman spectroscopy system is sent to the cloud server, where it can be accessed and analyzed through a web-based application](https://telnyx.com/resources/iot-remote-monitoring).

[**Advantages**](https://jascoinc.com/learning-center/theory/spectroscopy/confocal-raman-microscopy/)**:**

* Can be used for chemical or molecular analysis of unknown compounds in a small area, down to less than a micron.
* Can map areas of a sample, useful for samples with patterns or two different regions.
* Can perform depth profiling, allowing the user to see layers of a sample without sample preparation.
* Non-destructive and can be used with solids, liquids, or gases.
* No sample preparation needed.

[**Disadvantages**](https://eng.libretexts.org/Bookshelves/Materials_Science/TLP_Library_II/19%3A_Raman_Spectroscopy/19.9%3A_Advantages_and_Disadvantages):

* The Raman effect is very weak, which leads to low sensitivity, making it difficult to measure low concentrations of a substance.
* Can be swamped by fluorescence from some materials.
* Some materials might not yield strong Raman signals.
* There’s a potential risk of sample damage.
* The process can be relatively slow.

[**Cost**4](https://www.holmarc.com/confocal_micro_raman_spectrometer.php): The cost of a confocal micro-Raman spectroscopy system can vary, but one example found was priced at $35,400.00.

[**Scalability**5](https://journals.sagepub.com/doi/pdf/10.1366/000370209789379196)[6](https://opg.optica.org/ao/abstract.cfm?uri=ao-62-33-8724): Confocal Raman microscopy is scalable in terms of its ability to analyze different sample sizes, from microscopic to larger areas. It also has the potential for miniaturization and rapid imaging, as demonstrated by a MEMS-based portable confocal Raman spectroscopy system.

**Communication Technology** the IoT device communicates with the cloud server via Wi-Fi, allowing for remote monitoring and control of the system. The data collected by the confocal micro-Raman spectroscopy system is sent to the cloud server, where it can be accessed and analyzed through the web-based application.

**Potential Challenges** There could be several challenges in implementing this technology in Sri Lanka:

* [Infrastructure: There might be challenges related to setting up the necessary infrastructure, especially in remote areas where internet connectivity might be poor3](https://journals.sagepub.com/doi/pdf/10.1366/000370209789379196).
* [Cost: The cost of setting up the confocal micro-Raman spectroscopy system and the IoT devices might be high4](https://opg.optica.org/ao/abstract.cfm?uri=ao-60-27-8375).
* [Technical Expertise: There might be a lack of technical expertise in operating the confocal micro-Raman spectroscopy system and the IoT devices3](https://journals.sagepub.com/doi/pdf/10.1366/000370209789379196).
* [Maintenance: Regular maintenance of the system and the IoT devices might be challenging, especially in remote areas3](https://journals.sagepub.com/doi/pdf/10.1366/000370209789379196).

**References**

<https://opg.optica.org/ao/abstract.cfm?uri=ao-60-27-8375>

[Application of confocal laser Raman spectroscopy on marine sediment microplastics | Journal of Oceanology and Limnology (springer.com)](https://link.springer.com/article/10.1007/s00343-020-0129-z)


<https://www.bruker.com/en/products-and-solutions/infrared-and-raman/raman-microscopes/what-is-raman-microscopy.html>

<https://ijcrt.org/papers/IJCRT2303202.pdf>

* Visual Identification: A method involving the manual examination of samples under a microscope to identify microplastic particles based on their physical characteristics.



* Spectroscopy Techniques: These include methods like **FTIR (Fourier Transform Infrared Spectroscopy)** and **Raman Spectroscopy**, which analyze the chemical composition of particles to confirm the presence of microplastics.
* Chemical Analysis: Techniques such as **Pyrolysis-GC/MS (Pyrolysis Gas Chromatography/Mass Spectrometry)** that break down the samples into simpler compounds to identify the types of plastics.



* Density Separation: A process that separates microplastics from other materials based on their density differences, often using solutions like saline water.

The methodology across these methods involves collecting samples, preparing them for analysis, and then using one or more of the above techniques to identify and quantify microplastics. The choice of method depends on the sample type, the size of the microplastics, and the level of detail required for the analysis.

# **Validation and application of cost and time effective methods for the detection of 3–500 μm sized microplastics in the urban marine and estuarine environments**

**Microplastic Detection Process:**

* **Sample Collection:** This involves collecting water samples from various sources.
* **Digestion:** The collected samples undergo a process called digestion, where they are treated with hydrogen peroxide. [This helps to break down organic matter in the samples, making it easier to detect microplastics1](https://microplastics.springeropen.com/articles/10.1186/s43591-024-00081-x).
* **Microplastic Counting**: The samples are then examined for microplastics. [Two techniques were used in your example: unstained visual examination and Nile Red staining identification1](https://microplastics.springeropen.com/articles/10.1186/s43591-024-00081-x).
* [Unstained visual examination involves looking at the sample under a microscope without any added stains, while Nile Red staining uses a specific dye that binds to plastic, making the microplastics easier to see under a microscope1](https://microplastics.springeropen.com/articles/10.1186/s43591-024-00081-x).
* [I**ntegration with IoT Communication**:  The Internet of Things (IoT) can be used to enhance this process by providing real-time monitoring and data collection2](https://mondo.com/insights/iot-real-time-monitoring-transforming-industries/). For example, IoT sensors could be deployed in the water bodies to continuously collect samples and monitor microplastics. [These sensors could be connected to a central system that processes and analyzes the data in real time3](https://telnyx.com/resources/iot-remote-monitoring). This would allow for immediate detection and quantification of microplastics, enabling swift responses to changes in microplastic levels.

**Advantages:**

* [Real-time Monitoring: IoT integration allows for real-time monitoring and data collection1](https://doi.org/10.3390/). [This can lead to immediate detection and quantification of microplastics, enabling swift responses to changes in microplastic levels1](https://doi.org/10.3390/).
* [Large-scale Data Collection: IoT devices can be deployed in multiple locations, allowing for large-scale data collection1](https://doi.org/10.3390/).
* [Automation: The use of IoT reduces the need for manual sample collection and analysis, making the process more efficient1](https://doi.org/10.3390/).

**Disadvantages:**

* [Cost: The development and deployment of IoT devices can be expensive2](https://link.springer.com/article/10.1007/s13762-021-03384-1)[3](https://bnrc.springeropen.com/articles/10.1186/s42269-023-01148-0).
* [Infrastructure: Robust and reliable data transmission infrastructure is needed for IoT devices to function effectively1](https://doi.org/10.3390/)[4](https://doi.org/10.3390/environsciproc2021009029).
* [Complexity: Accurately detecting and quantifying microplastics is complex and can be challenging to implement in an IoT device5](https://link.springer.com/article/10.1007/s13762-023-05151-w).

[**Cost**: The cost of existing microplastic detection methods can range from $100 to $500 for sample collection tools6, and up to $30,000 for advanced systems like microscope-based spectroscopy systems6](https://finmodelslab.com/blogs/startup-costs/microplastic-detection-service-startup-costs). [The cost of implementing an IoT solution would likely be higher due to the cost of developing and deploying the IoT devices2](https://link.springer.com/article/10.1007/s13762-021-03384-1)[3](https://bnrc.springeropen.com/articles/10.1186/s42269-023-01148-0).

[**Feasibility:** While the technology for microplastic detection and IoT communication exists7](https://www.epa.gov/sciencematters/assessing-methods-measuring-microplastics-water)[8](https://microplastics.springeropen.com/articles/10.1186/s43591-024-00081-x)[1](https://doi.org/10.3390/)[4](https://doi.org/10.3390/environsciproc2021009029)[, implementing this solution on a large scale could present several challenges2](https://link.springer.com/article/10.1007/s13762-021-03384-1)[3](https://bnrc.springeropen.com/articles/10.1186/s42269-023-01148-0).

[**Suitability:** Existing microplastic detection methods have their own advantages and limitations2](https://link.springer.com/article/10.1007/s13762-021-03384-1)[9](https://link.springer.com/article/10.1134/S1061934822070127). [The suitability of integrating IoT would depend on the specific requirements of the use case9](https://link.springer.com/article/10.1134/S1061934822070127).

[**Availability:** Existing microplastic detection methods are widely available and have been used extensively in research2](https://link.springer.com/article/10.1007/s13762-021-03384-1)[3](https://bnrc.springeropen.com/articles/10.1186/s42269-023-01148-0)[5](https://link.springer.com/article/10.1007/s13762-023-05151-w). [The availability of an IoT integrated solution would depend on the development and deployment of the necessary IoT devices2](https://link.springer.com/article/10.1007/s13762-021-03384-1)

**Implementing IoT solutions in countries like Sri Lanka can face several challenges, but there are also ways to overcome these obstacles:**

**Challenges:**

* [Infrastructure: Sri Lanka requires significant investment in IoT infrastructure1](https://www.ft.lk/Columnists/Simple-sector-specific-IoT-solutions-to-drive-economic-value-in-Sri-Lanka-over-the-short-term/4-639982). [The key contributor to the IoT value chain is the platform, which requires a well-established IoT network infrastructure1](https://www.ft.lk/Columnists/Simple-sector-specific-IoT-solutions-to-drive-economic-value-in-Sri-Lanka-over-the-short-term/4-639982).
* [Regulations: Imported IoT solutions will likely have to conform to regulatory standards that vary according to country1](https://www.ft.lk/Columnists/Simple-sector-specific-IoT-solutions-to-drive-economic-value-in-Sri-Lanka-over-the-short-term/4-639982). [This can lead to significant complications during adoption1](https://www.ft.lk/Columnists/Simple-sector-specific-IoT-solutions-to-drive-economic-value-in-Sri-Lanka-over-the-short-term/4-639982).
* [Network Cooperation: Lack of network cooperation and transfer of innovation from scientific research institutions to practical practices can be a challenge2](http://dl.lib.uom.lk/bitstream/handle/123/21332/75-S15054.pdf?sequence=1).
* [Technical Expertise: There might be a lack of technical expertise in setting up and operating the IoT system3](https://www.sundaytimes.lk/230212/education/revolutionising-healthcare-in-sri-lanka-the-power-of-iot-in-transforming-medical-industry-511365.html).
* [Security: Ensuring the security and reliability of IoT-enabled devices and systems is also a major concern3](https://www.sundaytimes.lk/230212/education/revolutionising-healthcare-in-sri-lanka-the-power-of-iot-in-transforming-medical-industry-511365.html).

**References**

[**https://www.sciencedirect.com/science/article/abs/pii/S0025326X19302450**](https://www.sciencedirect.com/science/article/abs/pii/S0025326X19302450)

[**https://microplastics.springeropen.com/articles/10.1186/s43591-024-00081-x**](https://microplastics.springeropen.com/articles/10.1186/s43591-024-00081-x)

[**https://www.technologynetworks.com/applied-sciences/articles/microplastic-detection-353032**](https://www.technologynetworks.com/applied-sciences/articles/microplastic-detection-353032)

[**https://link.springer.com/article/10.1007/s11356-021-12943-5**](https://link.springer.com/article/10.1007/s11356-021-12943-5)